> # Launching FlexAttach in DCNM-SAN

> ## Detailed Steps

> To launch FlexAttach in DCNM-SAN, follow these steps:

> 1. In the Logical Domains pane, select a switch.
> 2. In the Physical Attributes pane, expand Switches > FC Services > N_Port Virtualizer (NPV) > Flex Attach.

> The FlexAttach configuration pane appears to the right.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.