> # Config

> Field | Description
> --- | ---
> FC Map | The FCoE Mac Address Prefix used to associate the FCoE Node (ENode).
> Default FCF Priority | The default FCoE Initialization Protocol (FIP) priority value advertised by the Fibre Channel Forwarder (FCF) to ENodes.
> FKA Adv. Period | The time interval at which FIP Keepalive (FKA) messages are transmitted to the MAC address of the ENode.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.