<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<!-- saved from url=(0014)about:internet -->
<html xmlns="http://www.w3.org/1999/xhtml" xml:lang="en" lang="en">
  <head>
    <meta http-equiv="Content-Type" content="text/html; charset=UTF-8" />
    <meta http-equiv="Content-Style-Type" content="text/css" />
    <meta name="GENERATOR" content="Quadralay WebWorks AutoMap 2003 Platinum Edition Client for FrameMaker 8.6.6597.0" />
    <meta name="TEMPLATEBASE" content="emwebh8-1-17" />
    <meta name="LASTUPDATED" content="08/01/13 14:45:16" />
    <title>IP Storage </title>
    <!-- Copyright 2010-2013, Cisco Systems, Inc. All rights reserved. -->

    <link rel="StyleSheet" href="document.css" type="text/css" />
    <link rel="StyleSheet" href="catalog.css" type="text/css" />


<script> 
    var is_chrome = navigator.userAgent.toLowerCase().indexOf('chrome') > -1; 
   
    if(is_chrome){document.domain=document.domain}
   </script>
    <script type="text/javascript" language="JavaScript1.2" src="expand.js"></script>
    <script type="text/javascript" language="JavaScript1.2" src="page.js"></script>

    <script type="text/javascript" language="JavaScript1.2">
     <!--
      function  WWNoOp() {}
      function  WWNoValue() { return ""; }

      var  VarDropDown;

      if (typeof(HTMLHelp_Object) != "undefined")
      {
        VarDropDown = new WWDropDown_Object();
      }
      else
      {
        VarDropDown = new Object();
        VarDropDown.fAnchorOpen  = WWNoOp;
        VarDropDown.fAnchorClose = WWNoOp;
        VarDropDown.fDIVOpen  = WWNoOp;
        VarDropDown.fDIVClose = WWNoOp;
      }
     // -->
    </script>

  
<SCRIPT language="javascript">
<!--
  self.document.write("<link href='"+top.relPath+"shared/style.css' rel='stylesheet' type='text/css'>");
  myid=197;
  self.document.write("<script type='text/javascript' language='JavaScript' src='"+top.relPath+"shared/con_utils.js'></scr"+"ipt>");
//-->
</SCRIPT>
</head>

  <body onload="highlightSearchTerms();" bgcolor="#ffffff">

    
    <blockquote>
    <a name="top"></a>

    
    


<a name="wp1047027"> </a><h1 class="pTitle">
IP Storage

</h1>
<a name="wp1047029"> </a><h1 class="pTitle">



FCIP Profiles

</h1>
<a name="wp1055580"> </a><p class="pBodyRelative">
</p><div>
<table border="2" cellpadding="2" id="wp1055517table1055515">
  <caption></caption>
  <tr bgcolor="#CCCCCC" align="left" valign="middle">    <th><a name="wp1055517"> </a><p class="pCellHeading">
Field 

</p>
</th>
    <th><a name="wp1055519"> </a><p class="pCellHeading">
Description 

</p>
</th>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055521"> </a><p class="pBody">
IP Address

</p>
</td>
    <td><a name="wp1055523"> </a><p class="pBody">
The Internet address for this entity.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055525"> </a><p class="pBody">
Port

</p>
</td>
    <td><a name="wp1055527"> </a><p class="pBody">
A TCP port other than the FCIP well-known port on which the FCIP 
entity listens for new TCP connection requests.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055529"> </a><p class="pBody">
SACK

</p>
</td>
    <td><a name="wp1055531"> </a><p class="pBody">
Whether the TCP Selective Acknowledgement Option is enabled to 
allow the receiver end to acknowledge multiple lost frames in a single 
ACK, enabling faster recovery.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055533"> </a><p class="pBody">
KeepAlive (s)

</p>
</td>
    <td><a name="wp1055535"> </a><p class="pBody">
The TCP keep alive timeout for all links within this entity.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055537"> </a><p class="pBody">
ReTrans MinTimeout (ms)

</p>
</td>
    <td><a name="wp1055539"> </a><p class="pBody">
The TCP minimum retransmit timeout for all the links on this entity.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055541"> </a><p class="pBody">
ReTrans Max

</p>
</td>
    <td><a name="wp1055543"> </a><p class="pBody">
The Maximum number of times that the same item of data will be 
retransmitted over a TCP connection. If delivery is not acknowledged 
after this number of retransmissions then the connection is terminated.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055545"> </a><p class="pBody">
Send BufSize (KB)

</p>
</td>
    <td><a name="wp1055547"> </a><p class="pBody">
The aggregate TCP send window for all TCP connections on all Links 
within this entity. This value is used for Egress Flow Control. When the 
aggregate of the data queued on all connections within this entity 
reaches this value, the sender is flow controlled.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055549"> </a><p class="pBody">
Bandwidth Max (Kb)

</p>
</td>
    <td><a name="wp1055551"> </a><p class="pBody">
This is an estimate of the Bandwidth of the network pipe used for the 
B-D product computation, which lets us derive the TCP receive window 
to advertise.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055553"> </a><p class="pBody">
Bandwidth Min (Kb)

</p>
</td>
    <td><a name="wp1055555"> </a><p class="pBody">
The minimum available bandwidth for the TCP connections on the Links 
within this entity.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055557"> </a><p class="pBody">
Est Round Trip Time (us)

</p>
</td>
    <td><a name="wp1055559"> </a><p class="pBody">
This is an estimate of the round trip delay of the network pipe used for 
the B-D product computation, which lets us derive the TCP receive 
window to advertise.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055561"> </a><p class="pBody">
PMTU Enable

</p>
</td>
    <td><a name="wp1055563"> </a><p class="pBody">
The path MTU discovery.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055565"> </a><p class="pBody">
PMTU ResetTimeout (sec)

</p>
</td>
    <td><a name="wp1055567"> </a><p class="pBody">
The time interval for which the discovered pathMTU is valid, before 
MSS reverts back to the negotiated TCP value.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055569"> </a><p class="pBody">
CWM Enable

</p>
</td>
    <td><a name="wp1055571"> </a><p class="pBody">
If true, congestion window monitoring is enabled.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055573"> </a><p class="pBody">
CWM BurstSize (KB)

</p>
</td>
    <td><a name="wp1055575"> </a><p class="pBody">
The maximum burst sent after a TCP sender idle period.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1055577"> </a><p class="pBody">
Max Jitter

</p>
</td>
    <td><a name="wp1055579"> </a><p class="pBody">
The maximum delay variation (not due to congestion) that can be 
experienced by TCP connections on this interface.

</p>
</td>
</tr>
</table>
</div>
<p class="pBodyRelative">
</p>
<hr /><br><p class="pBody">Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.</p> 

    </blockquote>

  </body>
</html>
