> # CFS Protocol

> The CFS functionality is independent of the lower layer transport. Currently, in Cisco MDS switches, the CFS protocol layer resides on top of the Fiber Channel 2 (FC2) layer and is peer-to-peer with no client-server relationship. CFS uses the FC2 transport services to send information to other switches. CFS uses a proprietary SW_ILS (0x77434653) protocol for all CFS packets. CFS packets are sent to or from the switch domain controller addresses.

> CFS can also use IP to send information to other switches.

> Applications that use CFS are completely unaware of the lower layer transport.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.