> # Virtual FC Interface Monitor Traffic

> The Monitor dialog boxes have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> RxBytes | The number of bytes, including the frame delimiters, received by this port from its attached N_Port.
> RxFrames | The number of frames, including the frame delimiters, received by this port from its attached N_Port.
> TxBytes | The number of bytes, including the frame delimiters, transmitted by this port to its attached N_Port.
> TxFrames | The number of frames, including the frame delimiters, transmitted by this port to its attached N_Port.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.