> # SANTap DVT

> Field | Description
> --- | ---
> VSAN Id, Port WWN | Represents the port world wide name of the created DVT. It will be the same as the port world wide name of the real target for which data is to be replicated.
> Interface | Represents the port on the module where the DVT will be created.
> Target VSAN Id | Represents the VSAN of the real target for which this DVT is being created.
> Name | The administratively assigned name for this DVT.
> LUNSize Handling | Indicates whether the DVT should use the real target LUN size for the virtual LUN or the max LUN size supported which is 2TB.
> IO Timeout (sec) | Represents the IO timeout value associated with the DVT. This object should be set during the DVT creation time and cannot be modified later.
> Target IO Timeout (sec) | Represents the target IO timeout value associated with the DVT.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.