> # Configuring an HTTP Proxy Server

> ## Detailed Steps

> To configure a Call Home HTTP proxy server, follow these steps:

> 1. Select a switch in the Fabric pane.
> 2. Expand Events, select Call Home, and HTTP Proxy Server in the Physical Attributes pane.

> You see the Call Home HTTP Proxy Server information in the Information pane.

> 3. Click the Address Type tab.

> The Address Type options are displayed.

> 4. Click the Address tab and enter the address of the HTTP proxy server.
> 5. Click the Port tab and enter a integer number to specify the port of the HTTP proxy server.
> 6. Check the Enable check box to enable the HTTP proxy configured for Call Home.
> 7. (Optional) Set an empty value in the Address tab to delete the HTTP proxy server from the MDS switch.
> 8. Choose an address type. You can select ipv4, ipv6, or DNS.

> Note If the address is empty, then no proxy server is configured.

> 1. Click Apply to update HTTP Proxy Server options.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.