> # Setting the Call Home Message Levels

> ## Restrictions

> - The urgency level ranges from 0 (lowest level of urgency) to 9 (highest level of urgency), and the default is 0 (all messages are sent).

> ## Detailed Steps

> To set the message level for each destination profile for Call Home, follow these steps:

> 1. Expand Events and select Call Home in the Physical Attributes pane.

> You see the Call Home information in the Information pane.

> In Device Manager, choose Admin > Events > Call Home.

> 2. Click the Profiles tab in the Information Pane.

> You see the Call Home profiles.

> 3. Set a message level for each switch using the drop-down menu in the MsgLevel column.
> 4. Click the Apply Changes icon to save your changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.