> # Creating Static Mapping

> ## Detailed Steps

> To create a static iSCSI virtual target for the entire Fibre Channel target port using Device Manager, follow these steps:

> 1. Click IP > iSCSI.

> You see the iSCSI configuration.

> 2. Click the Targets tab to display a list of existing iSCSI targets .
> 3. Click Create to create an iSCSI target.

> You see the Create iSCSI Targets dialog box.

> 4. Set the iSCSI target node name in the iSCSI Name field, in IQN format.
> 5. Set the Port WWN field for the Fibre Channel target port you are mapping.
> 6. Click the Select from List radio button and set the iSCSI initiator node names or IP addresses that you want this virtual iSCSI target to access, or click the All radio button to let the iSCSI target access all iSCSI initiators. Also see the "iSCSI Access Control" topic.
> 7. Click the Select from List radio button and check each interface you want to advertise the iSCSI targets on or click the All radio button to advertise all interfaces.
> 8. Click Apply to save this change.

> Tip An iSCSI target cannot contain more than one Fibre Channel target port. If you have already mapped the whole Fibre Channel target port, you cannot use the LUN mapping option.

> Note See the "iSCSI-Based Access Control" topic for more information on controlling access to statically mapped targets.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.