> # Configuring the RSCN Timer with CFS

> ## Detailed Steps

> To configure the RSCN timer with CFS, follow these steps:

> 1. Expand a fabric, expand a VSAN, and then select Advanced in the Logical Domains pane.
> 2. Click the RSCN Event tab.

> You see the VSAN advanced configuration in the Information pane.

> 3. Double-click the TimeOut value to change the value (in milliseconds) for the selected VSAN.
> 4. Click Apply Changes to save these changes, or click Undo Changes to cancel any unsaved changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.