> # Enabling Enhanced Zoning

> By default, the enhanced zoning feature is disabled in all switches in the Cisco MDS 9000 Family.

> ## Detailed Steps

> To enable enhanced zoning in a VSAN, follow these steps:

> 1. Expand a VSAN and then select a zone set in the Logical Domains pane.

> You see the zone set configuration in the Information pane.

> 2. Click the Enhanced tab.

> You see the current enhanced zoning configuration.

> 3. From the Action drop-down menu, choose enhanced to enable enhanced zoning in this VSAN.
> 4. Click Apply Changes to save these changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.