<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<!-- saved from url=(0014)about:internet -->
<html xmlns="http://www.w3.org/1999/xhtml" xml:lang="en" lang="en">
  <head>
    <meta http-equiv="Content-Type" content="text/html; charset=UTF-8" />
    <meta http-equiv="Content-Style-Type" content="text/css" />
    <meta name="GENERATOR" content="Quadralay WebWorks AutoMap 2003 Platinum Edition Client for FrameMaker 8.6.6597.0" />
    <meta name="TEMPLATEBASE" content="emwebh8-1-17" />
    <meta name="LASTUPDATED" content="08/01/13 14:48:13" />
    <title>VRRP General </title>
    <!-- Copyright 2010-2013, Cisco Systems, Inc. All rights reserved. -->

    <link rel="StyleSheet" href="document.css" type="text/css" />
    <link rel="StyleSheet" href="catalog.css" type="text/css" />


<script> 
    var is_chrome = navigator.userAgent.toLowerCase().indexOf('chrome') > -1; 
   
    if(is_chrome){document.domain=document.domain}
   </script>
    <script type="text/javascript" language="JavaScript1.2" src="expand.js"></script>
    <script type="text/javascript" language="JavaScript1.2" src="page.js"></script>

    <script type="text/javascript" language="JavaScript1.2">
     <!--
      function  WWNoOp() {}
      function  WWNoValue() { return ""; }

      var  VarDropDown;

      if (typeof(HTMLHelp_Object) != "undefined")
      {
        VarDropDown = new WWDropDown_Object();
      }
      else
      {
        VarDropDown = new Object();
        VarDropDown.fAnchorOpen  = WWNoOp;
        VarDropDown.fAnchorClose = WWNoOp;
        VarDropDown.fDIVOpen  = WWNoOp;
        VarDropDown.fDIVClose = WWNoOp;
      }
     // -->
    </script>

  
<SCRIPT language="javascript">
<!--
  self.document.write("<link href='"+top.relPath+"shared/style.css' rel='stylesheet' type='text/css'>");
  myid=2071;
  self.document.write("<script type='text/javascript' language='JavaScript' src='"+top.relPath+"shared/con_utils.js'></scr"+"ipt>");
//-->
</SCRIPT>
</head>

  <body onload="highlightSearchTerms();" bgcolor="#ffffff">

    
    <blockquote>
    <a name="top"></a>

    
    


<a name="wp1096848"> </a><h1 class="pTitle">



VRRP General

</h1>
<a name="wp1096893"> </a><p class="pBodyRelative">
</p><div>
<table border="2" cellpadding="2" id="wp1096851table1096849">
  <caption></caption>
  <tr bgcolor="#CCCCCC" align="left" valign="middle">    <th><a name="wp1096851"> </a><p class="pCellHeading">
Field 

</p>
</th>
    <th><a name="wp1096853"> </a><p class="pCellHeading">
Description 

</p>
</th>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096855"> </a><p class="pBody">
IP Address Type, VrId, 
Interface

</p>
</td>
    <td><a name="wp1096857"> </a><p class="pBody">
The IP address type (IPv4, IPv6, or DNS), the virtual router ID, and the 
interface.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096859"> </a><p class="pBody">
Admin

</p>
</td>
    <td><a name="wp1096861"> </a><p class="pBody">
The admin state of the virtual router (active or notInService).

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096863"> </a><p class="pBody">
Oper

</p>
</td>
    <td><a name="wp1096865"> </a><p class="pBody">
The current state of the virtual router. There are three defined values:

</p>
<div class="pSmartList1"><ul class="pSmartList1">
<a name="wp1096866"> </a><li class="pSmartList1">initialize&#8212; Indicates that all the virtual router is waiting for a 
startup event.
</li>
<a name="wp1096867"> </a><li class="pSmartList1">backup&#8212; Indicates the virtual router is monitoring the availability 
of the master router.
</li>
<a name="wp1096868"> </a><li class="pSmartList1">master&#8212; Indicates that the virtual router is forwarding frames for 
IP addresses that are associated with this router.
</li>
</ul></div>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096870"> </a><p class="pBody">
Priority

</p>
</td>
    <td><a name="wp1096872"> </a><p class="pBody">
Specifies the priority to be used for the virtual router master election 
process. Higher values imply higher priority. A priority of 0 is sent by 
the master router to indicate that this router has ceased to participate in 
VRRP and a backup virtual router should transition to become a new 
master. A priority of 255 is used for the router that owns the associated 
IP address(es).

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096874"> </a><p class="pBody">
AdvInterval

</p>
</td>
    <td><a name="wp1096876"> </a><p class="pBody">
The time interval, in seconds, between sending advertisement messages. 
Only the master router sends VRRP advertisements.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096878"> </a><p class="pBody">
PreemptMode

</p>
</td>
    <td><a name="wp1096880"> </a><p class="pBody">
Controls whether a higher priority virtual router will preempt a lower 
priority master.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096882"> </a><p class="pBody">
UpTime

</p>
</td>
    <td><a name="wp1096884"> </a><p class="pBody">
When this virtual router transitioned out of initialized.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096886"> </a><p class="pBody">
Version

</p>
</td>
    <td><a name="wp1096888"> </a><p class="pBody">
The VRRP version on which this VRRP instance is running.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1096890"> </a><p class="pBody">
AcceptMode

</p>
</td>
    <td><a name="wp1096892"> </a><p class="pBody">
Controls whether a virtual router in Master state will accept packets 
addressed to the address owner&#39;s IPv6 address as its own if it is not the 
IPv6 address owner. If true, the virtual router in Master state will accept. 
If false, the virtual router in Master state will not accept.

</p>
</td>
</tr>
</table>
</div>
<p class="pBodyRelative">
</p>
<hr /><br><p class="pBody">Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.</p> 

    </blockquote>

  </body>
</html>
