> # Configuring SCSI Flow Services

> This section includes the following topics:

> - Enabling Intelligent Storage Services
> - Configuring Fibre Channel Using DCNM-SAN
> - Disabling Intelligent Storage Services

> ## Restrictions <Optional>

> Enabling SCSI flow services on interfaces has the following restrictions:

> - The fewest number of interfaces that you can enable is four. You can specify fc1 through fc4, but not fc1 through fc2.
> - The first interface in the group must be 1, 5, 9, 13, 17, 21, 25, or 29. You can specify fc5 through fc8, but not fc7 through fc10.
> - The groups of four interfaces do not need to be consecutive. You can specify fc1 through fc8 and fc17 through fc20.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.