> # Configuring iSCSI

> Cisco MDS 9000 Family IP storage (IPS) services extend the reach of Fibre Channel SANs by using open-standard, IP-based technology. The switch allows IP hosts to access Fibre Channel storage using the iSCSI protocol.

> Note The iSCSI feature is specific to the IPS module and is available in Cisco MDS 9200 Switches or Cisco MDS 9500 Directors.
> The Cisco MDS 9216i switch and the 14/2 Multiprotocol Services (MPS-14/2) module also allow you to use Fibre Channel, FCIP, and iSCSI features. The MPS-14/2 module is available for use in any switch in the Cisco MDS 9200 Series or Cisco MDS 9500 Series.

> Note For information on configuring Gigabit Ethernet interfaces, see "Configuring Gigabit Ethernet Interface" topic.

> This chapter includes the following topics:

> - Information About iSCSI
> - Licensing Requirements for iSCSI
> - Guidelines and Limitations
> - Default Settings
> - Configuring iSCSI
> - Configuring iSLB
> - Distributing the iSLB Configuration Using CFS
> - Configuring iSCSI Authentication
> - Creating an iSNS Client Profile
> - Configuring iSNS Cloud Discovery
> - Field Descriptions for iSCSI
> - Additional References

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.