> # Configuring Broadcast Zoning

> ## Detailed Steps

> To broadcast frames in the basic zoning mode, follow these steps:

> 1. Expand a VSAN and then select a zone set in the Logical Domains pane.
> 2. Click the Policies tab in the Information pane.

> You see the Zone policy information in the Information pane.

> 3. Check the Broadcast check box to enable broadcast frames on the default zone.
> 4. Click Apply Changes to save these changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.