> # Information About Control Traffic

> The Cisco MDS 9000 Family supports QoS for internally and externally generated control traffic. Within a switch, control traffic is sourced to the supervisor module and is treated as a high priority frame. A high priority status provides absolute priority over all other traffic and is assigned in the following cases:

> - Internally generated time-critical control traffic (mostly Class F frames).
> - Externally generated time-critical control traffic entering a switch in the Cisco MDS 9000 Family from a another vendor’s switch. High priority frames originating from other vendor switches are marked as high priority as they enter a switch in the Cisco MDS 9000 Family.

> The Cisco MDS 9000 Family supports QoS for internally and externally generated control traffic. Within a switch, control traffic is sourced to the supervisor module and is treated as a high priority frame. A high priority status provides absolute priority over all other traffic and is assigned in the following cases:

> - Internally generated time-critical control traffic (mostly Class F frames).
> - Externally generated time-critical control traffic entering a switch in the Cisco MDS 9000 Family from a another vendor’s switch. High priority frames originating from other vendor switches are marked as high priority as they enter a switch in the Cisco MDS 9000 Family.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.