> # iSNS Configuration Distribution

> You can use the CFS infrastructure to distribute the iSCSI initiator configuration to iSNS servers across the fabric. This allows the iSNS server running on any switch to provide a querying iSNS client a list of iSCSI devices available anywhere on the fabric. For information on CFS, see the System Management Configuration Guide, Cisco DCNM for SAN.

> ## Detailed Steps

> To enable iSNS configuration distribution, follow these steps:

> 1. Choose End Devices > iSNS.

> You see the iSNS configuration in the Information pane.

> 2. Click the CFS tab and select enable from the Admin drop-down menu for iSNS.
> 3. Select enable from the Global drop-down menu for iSNS.
> 4. Click the Apply Changes icon to save this change.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.