> # Setting QoS Values

> ## Detailed Steps

> To set the QoS values, follow these steps:

> 1. Expand Switches, expand FC Interfaces, and then select Logical in the Physical Attributes pane.

> You see the Interface tables in the Information pane.

> 2. In Device Manager, choose Interface > Ethernet and iSCSI.

> You see the Ethernet Interfaces and iSCSI dialog box.

> 3. Click the iSCSI TCP tab in either Cisco DCNM-SAN or Device Manager.

> You see the iSCSI TCP configuration table.

> 4. Set the QoS field from 1 to 6.
> 5. Click the Apply Changes icon in Cisco DCNM-SAN or click Apply in Device Manager to save these changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.