> # Diagnostics

> Field | Description
> --- | ---
> Value | Displays the most recent measurement seen by the sensor.
> Alarms High and Low | Represents the severity level of the SFP diagnostic information of an interface for temperature, voltage, current, optical transmit and receive power. It ranges from 1 to 6, with 6 being highest severity.
> Warnings High and Low

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.