> # VRRP Statistics

> Field | Description
> --- | ---
> IP Address Type, VrId, Interface | The IP address type (IPv4, IPv6, or DNS), the virtual router ID, and the interface.
> LastAdvRx | The total number of VRRP advertisements received by this virtual router.
> Protocol Traffic MasterIpAddr | The master router's real (primary) IP address. This is the IP address listed as the source in VRRP advertisement last received by this virtual router.
> Protocol Traffic BecomeMaster | The total number of times that this virtual router's state has transitioned to MASTER.
> Priority 0 Rx | The total number of VRRP frames received by the virtual router with a priority of 0.
> Priority 0Tx | The total number of VRRP frames sent by the virtual router with a priority of 0.
> AuthErrors InvalidType | The total number of frames received with an unknown authentication type.
> Other Errors dvIntervalErrors | The total number of VRRP advertisement frames received for which the advertisement interval is different than the one configured for the local virtual router.
> Other Errors IpTtlErrors | The total number of VRRP frames received by the virtual router with IP TTL (time-to-live) not equal to 255.
> Other Errors InvalidTypePktsRcvd | The number of VRRP frames received by the virtual router with an invalid value in the type field.
> Other Errors AddressListErrors | The total number of frames received for which the address list does not match the locally configured list for the virtual router.
> OtherErrors PacketLengthErrs | The total number of frames received with a frame length less than the length of the VRRP header.
> RefreshRate | The interval of time between refreshes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.