> # Configuring Zone-Based Traffic Priority

> ## Detailed Steps

> To configure the zone priority, follow these steps:

> 1. Expand a VSAN and then select a zone set in the Logical Domains pane.
> 2. Click the Policies tab in the Information pane.

> You see the Zone policy information in the Information pane.

> 3. Use the check boxes and drop-down menus to configure QoS on the default zone.
> 4. Click Apply Changes to save the changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.