> # Selecting the Key Manager and SSL Settings

> 1. From the menu bar, select Config>Provision.

> The Key Manager Settings window is displayed with the following options:

> - None-No Key Manager selected for SME.
> - Cisco-Cisco Key Manager selected for SME.
> - RSA-RSA Key Manager selected for SME

> Note Once you have selected a Key Manager, you will not be able to change it.

> 1. Select one of the Radio buttons and click Submit Settings.

> The Key Manager Settings window is displayed.

> The KMC SSL Settings pane displays the location where the certificate is stored.

> 2. If you want to edit the SSL Settings, click Edit SSL Settings.
> 3. Use the drop-down to select the SME KMC Trust Certificate.
> 4. Use the drop-down to select the SME KMC Server Certificate.
> 5. Specify and confirm the Server Cert Password.
> 6. Click Submit SSL Settings.
> 7. In the High Availability Settings pane, click Edit HA Settings to specify the KMC Role of this Server and SME Secondary Server Address.
> 8. Click Submit HA Settings to confirm.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.