> # About Flow Statistics

> If you enable flow counters, you can enable a maximum of 1 K entries for aggregate flow and flow statistics for Generation 1 modules, and 2 K entries for Generation 2 modules. Be sure to assign an unused flow index to a module for each new flow. Flow indexes can be repeated across modules. The number space for flow index is shared between the aggregate flow statistics and the flow statistics.

> Generation 1 modules allow a maximum of 1024 flow statements per module. Generation 2 modules allow a maximum of 2048-128 flow statements per module.

> Note For each session, fcflow counter will increment only on locally connected devices and should be configured on the switch where the initiator is connected.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.