> # SPAN Sessions

> Field | Description
> --- | ---
> Dest Interface | The Span Destination port interface.
> Filter VSAN List | The VSANs that are assigned to this session.
> Status Admin | Suspend an active session or activate an inactive session.
> Status Oper | The current state of the session.
> Description | The description of the session status.
> VSAN List | The VSANs that are assigned to this session.
> Or Interface (Direction) | The destination port ID to be configured for the session.
> Inactive Reason | Description of the reason why this session is not active.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.