> # Saving a Customized Topology Map Layout

> Changes made to the topology map can be saved so that the customized view is available any time you open the DCNM-SAN Client for that fabric.

> ## DETAILED STEPS

> 1. Click File > Preferences to open the DCNM-SAN preferences dialog box.
> 2. Click the Map tab and check the Automatically Save Layout check box to save any changes to the topology map .
> 3. Click Apply, and then click OK to save this change.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.