> # RMON Thresholds 32bit Alarms

> Field | Description
> --- | ---
> Interval | The interval in seconds over which the data is sampled and compared with the rising and falling thresholds. When setting this variable, care should be taken in the case of deltaValue sampling - the interval should be set short enough that the sampled variable is very unlikely to increase or decrease by more than 2^31 - 1 during a single sampling interval.
> Variable | The variable to be sampled. Only variables that resolve to an ASN.1 primitive type of INTEGER (INTEGER, Integer32, Counter32, Counter64, Gauge, or TimeTicks) may be sampled.
> SampleType | The method of sampling the selected variable and calculating the value to be compared against the thresholds.
> Value | The value of the statistic during the last sampling period.
> StartupAlarm | The alarm that may be sent when this entry is first set to valid.
> Rising Threshold | A threshold for the sampled statistic. When the current sampled value is greater than or equal to this threshold, and the value at the last sampling interval was less than this threshold, a single event will be generated.
> Rising EventId | The ID of the eventEntry that is used when a rising threshold is crossed.
> Falling Threshold | A threshold for the sampled statistic. When the current sampled value is less than or equal to this threshold, and the value at the last sampling interval was greater than this threshold, a single event will be generated.
> Falling EventId | The ID of the eventEntry that is used when a falling threshold is crossed.
> FailedAttempts | The number of times the alarm variable was polled (in the active state) and no response was received.
> Owner | The ID of the user who configured this entry.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.