> # FCIP Monitor

> Field | Description
> --- | ---
> C3 Rx Bytes | The number of incoming bytes of data traffic.
> C3 Tx Bytes | The number of outgoing bytes of data traffic.
> CF Rx Bytes | The number of incoming bytes of control traffic.
> CF Tx Bytes | The number of outgoing bytes of control traffic.
> Rx Error | The number of inbound frames that contained errors preventing them from being deliverable to a higher-layer protocol.
> Tx Error | The number of outbound frames that could not be transmitted because of errors.
> RxDiscard | The number of inbound frames that were chosen to be discarded even though no errors had been detected to prevent their being deliverable to a higher-layer protocol.
> TxDiscard | The number of outbound frames that were chosen to be discarded even though no errors had been detected to prevent their being transmitted.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.