> # Configuring Management Interfaces

> ## Detailed Steps

> To configure the management interface using DCNM-SAN, follow these steps:

> 1. Select a VSAN in the Logical Domains pane.
> 2. In the Physical Attributes pane, expand Switches > Management.

> You see the interface configuration in the Information pane.

> 3. Click the IP Addresses tab and set the Interface, IP Address/Mask field.
> 4. Click the General tab and set the Status Admin to up.
> 5. (Optional) Set other configuration parameters using the other tabs.
> 6. Click Apply Changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.