> # Configuring RMON

> RMON is disabled by default, and no events or alarms are configured in the switch.

> This section includes the following topics:

> - Enabling RMON Alarms by Port
> - Enabling 32-Bit and 64-Bit Alarms
> - Creating RMON Alarms
> - Enabling 32-Bit RMON Alarms for VSANs
> - Enabling 32-Bit and 64-Bit RMON Alarms for Physical Components
> - Creating a New RMON from Device Manager Threshold Manager
> - Managing RMON Events
> - Managing RMON Alarms
> - Viewing the RMON Log

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.