> # About fctimer Distribution

> You can enable per-VSAN fctimer fabric distribution for all Cisco MDS switches in the fabric. When you perform fctimer configurations, and distribution is enabled, that configuration is distributed to all the switches in the fabric.

> You automatically acquire a fabric-wide lock when you issue the first configuration command after you enabled distribution in a switch. The fctimer application uses the effective and pending database model to store or commit the commands based on your configuration.

> Refer to the Cisco MDS 9000 Family NX-OS System Management Configuration Guide for more information on the CFS application.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.