> # Configuring Smart Zoning

> ## Detailed Steps

> To configure smart zoning, follow these steps:

> 1. Expand a VSAN and then select a zone set in the Logical Domains pane.
> 2. Click the Smart Zoning tab in the Information pane.

> You see the smart zoning information in the Information pane.

> 3. You can view the details under the Switch, Status, Command, Last Command, and Result headings.
> 4. You can set the Status, and Command fields.
> 5. Click Apply Changes to save these changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.