> # Management Interfaces

> You can remotely configure the switch through the management interface (mgmt0). To configure a connection on the mgmt0 interface, you must configure either the IP version 4 (IPv4) parameters (IP address, subnet mask, and default gateway) or the IP version 6 (IPv6) parameters so that the switch is reachable.

> Before you begin to configure the management interface manually, obtain the switch’s IPv4 address and subnet mask, or the IPv6 address.

> The management port (mgmt0) is autosensing and operates in full-duplex mode at a speed of 10/100/1000 Mbps. Autosensing supports both the speed and the duplex mode. On a Supervisor-1 module, the default speed is 100 Mbps and the default duplex mode is auto. On a Supervisor-2 module, the default speed is auto and the default duplex mode is auto.

> Note You need to explicitly configure a default gateway to connect to the switch and send IP packets or add a route for each subnet.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.