> # Configuring Load Balancing

> ## Detailed Steps

> To configure load balancing on an existing VSAN, follow these steps:

> 1. Choose Fabricxx > All VSAN s from the Logical Domains pane.

> You see the VSAN configuration in the Information pane.

> 2. Select a VSAN and complete the LoadBalancing field.
> 3. Click Apply Changes to save these changes, or click Undo Changes to discard any unsaved changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.