> # iSNS Cloud Discovery

> Field | Description
> --- | ---
> AutoDiscovery | Whether automatic cloud discovery is turned on or off.
> DiscoveryDelay | Time duration between successive IP cloud discovery runs.
> Discovery | The IP network discovery command to be executed. all - Run IP network discovery for all the gigabit ethernet interfaces in the fabric. noOp (default) - no operation is performed.
> CommandStatus | The status of the license install / uninstall / update operation. success - discovery operation completed successfully nProgress - discovery operation is in progress none - no discovery operation is performed NoIpNetworkNameSpecified - ipCloud name not specified invalidNetworkName - ipCloud is not configured NoIPSPortNameSpecified - gigE port ifindex not specified invalidIPSPortName - invalid gigE port interface generalISNSFailure - General ISNS Server Failure

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.