> # iSNS Details iSCSI Nodes

> Field | Description
> --- | ---
> Name | The iSCSI Name of the initiator or target associated with the storage node.
> Type | The Node Type bit-map defining the functions of this iSCSI node, where 31 is a Target, 30 is an Initiator, 29 is a Control, and all others are reserved.
> Alias | The Alias name of the iSCSI node.
> ScnBitmap | The State Change Notification (SCN) bitmap for a node.
> WWN Token | An optional globally unique 64-bit integer value that can be used to represent the World Wide Node Name of the iSCSI device in a Fibre Channel fabric.
> AuthMethod | The iSCSI authentication method enabled for this iSCSI Node.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.