> # Zoneset Policies

> Field | Description
> --- | ---
> Default Zone Behavior | Controls the behavior of the default zone on this VSAN. If it is set to permit, then the members of the default zone on this VSAN can communicate with each other. If it is set to deny, then the members of the default zone on this VSAN cannot communicate with each other.
> Default Zone ReadOnly | Indicates whether SCSI read operations are allowed on members of the default zone which are SCSI targets, on this VSAN. If true, then only SCSI read operations are permitted. So, this default zone becomes a read-only default zone on this VSAN. If false, then both SCSI read and write operations are permitted.
> Default Zone QoS | Specifies whether the QoS attribute for the default zone on this VSAN is enabled. If true, then QoS attribute for the default zone on this VSAN is enabled. If false, then the QoS attribute for the default zone on this VSAN is disabled.
> Default Zone QoS Priority | Specifies the QoS priority value.
> Default Zone Broadcast | Specifies if broadcast zoning is enabled on this default zone on this VSAN. If true, then it is enabled. If false, then it is disabled.
> Propagation | Controls the way zoneset information is propagated during Merge/Change protocols on this VSAN
> Read From | Specifies whether the management station wishes to read from the effective database or from the copy database.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.