Edge Ports View

Edge Ports view provides a view of the leaf nodes as VPC pairs. The visualization provides an interface similar to Fabric Path Links view but with details specific to VPC feature.

Each leaf is shown as paired with its VPC peer, with the line between the pair indicating the VPC link. The numbers on the nodes indicate the number of edge ports down for that node.

The color of the circle depends on the status of the edge ports or the status of the switch.

Clicking on a node selects the node and its peer (if any) and shows the edge port status details for that node in the left side panel, as shown below.

On Selecting a single VPC pair, specific information about the VPC setup such as VPC domain ID, VPC peer names, VPC consistency state, VPC Peerlink consistency, Primary VPC Port Channel ID, VPC role for each peer, primary VPC peer link ID, Secondary VPC port channel ID and secondary VPC peerlink ID are all displayed in a short table above the interface listing.

No specific information is overloaded on the link colors, since the link is intended to represent both the Peer link and the keep alive link between peers