## Adding a Network

1. From the menu bar, select Config > Auto-Configuration > Networks >Add.

2. In the Add Network window, use the drop-down to select the Organization and Partition.

Note If there is only one organization and partition configured, the values for these fields are automatically populated.

3. Specify the VRF Name for the partition.

The VRF Name must be of the format organizationName:partitionName.

4. Specify the Network Name to identify the network.

5. Specify the Multicast Group Address.

Note The Multicast Group Address is used to Enable VxLAN Encapsulation on the Admin > Fabric Encapsulation Settings page.

6. Select the Network Role from the drop-down list based on the type of the network.

7. In the Network ID section, choose one of the following:

• Segment ID Only

– Specify the Segment ID for the network.

• Mobility Domain and VLAN

– Specify the Segment ID for your network.

– Select Generate Seg ID to generate segment ID automatically.

– Specify the VLAN ID and Mobility Domain ID if you need to create a VLAN + Mobility Domain network.

8. In the DHCP Scope section, specify the IP Range.

9. Use the drop-down to select the Profile.

10. Specify the Profile parameters.

11. Specify the Service Configuration parameters.

12. Click Add.