> # Information About Fabric Binding

> The fabric binding feature ensures ISLs are only enabled between specified switches in the fabric binding configuration. Fabric binding is configured on a per-VSAN basis.

> This feature helps prevent unauthorized switches from joining the fabric or disrupting current fabric operations. It uses the Exchange Fabric Membership Data (EFMD) protocol to ensure that the list of authorized switches is identical in all switches in the fabric.

> This section inludes the following topics:

> - Port Security Versus Fabric Binding
> - Fabric Binding Enforcement

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.