> # Configuring Default Zone QoS Priority Attributes

> QoS priority attribute configuration changes take effect when you activate the zone set of the associated zone.

> Note If a member is part of two zones with two different QoS priority attributes, the higher QoS value is implemented. This situation does not arise in the VSAN-based QoS as the first matching entry is implemented.

> ## Detailed Steps

> To configure the QoS priority attributes for a default zone, follow these steps:

> 1. Choose Zone > Edit Local Full Zone Database.

> You see the Select VSAN dialog box.

> 2. Select a VSAN and click OK.

> You see the Edit Local Full Zone Database dialog box for the selected VSAN.

> 3. Choose Edit > Edit Default Zone Attributes to configure the default zone QoS priority attributes.
> 4. Check the Permit QoS Traffic with Priority check box and set the Qos Priority drop-down menu to low, medium, or high.
> 5. Click OK to save these changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.