> # FCIP and VE Ports

> FCIP virtual E (VE) ports behave exactly like standard Fibre Channel E ports, except that the transport in this case is FCIP instead of Fibre Channel. The only requirement is for the other end of the VE port to be another VE port.

> A virtual ISL is established over an FCIP link and transports Fibre Channel traffic. Each associated virtual ISL looks like a Fibre Channel ISL with either an E port or a TE port at each end.

> See the "Configuring B Ports" topic for more information.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.