<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<!-- saved from url=(0014)about:internet -->
<html xmlns="http://www.w3.org/1999/xhtml" xml:lang="en" lang="en">
  <head>
    <meta http-equiv="Content-Type" content="text/html; charset=UTF-8" />
    <meta http-equiv="Content-Style-Type" content="text/css" />
    <meta name="GENERATOR" content="Quadralay WebWorks AutoMap 2003 Platinum Edition Client for FrameMaker 8.6.6597.0" />
    <meta name="TEMPLATEBASE" content="emwebh8-1-17" />
    <meta name="LASTUPDATED" content="08/01/13 14:47:45" />
    <title>About Interop Mode </title>
    <!-- Copyright 2010-2013, Cisco Systems, Inc. All rights reserved. -->

    <link rel="StyleSheet" href="document.css" type="text/css" />
    <link rel="StyleSheet" href="catalog.css" type="text/css" />


<script> 
    var is_chrome = navigator.userAgent.toLowerCase().indexOf('chrome') > -1; 
   
    if(is_chrome){document.domain=document.domain}
   </script>
    <script type="text/javascript" language="JavaScript1.2" src="expand.js"></script>
    <script type="text/javascript" language="JavaScript1.2" src="page.js"></script>

    <script type="text/javascript" language="JavaScript1.2">
     <!--
      function  WWNoOp() {}
      function  WWNoValue() { return ""; }

      var  VarDropDown;

      if (typeof(HTMLHelp_Object) != "undefined")
      {
        VarDropDown = new WWDropDown_Object();
      }
      else
      {
        VarDropDown = new Object();
        VarDropDown.fAnchorOpen  = WWNoOp;
        VarDropDown.fAnchorClose = WWNoOp;
        VarDropDown.fDIVOpen  = WWNoOp;
        VarDropDown.fDIVClose = WWNoOp;
      }
     // -->
    </script>

  
<SCRIPT language="javascript">
<!--
  self.document.write("<link href='"+top.relPath+"shared/style.css' rel='stylesheet' type='text/css'>");
  myid=1487;
  self.document.write("<script type='text/javascript' language='JavaScript' src='"+top.relPath+"shared/con_utils.js'></scr"+"ipt>");
//-->
</SCRIPT>
</head>

  <body onload="highlightSearchTerms();" bgcolor="#ffffff">

    
    <blockquote>
    <a name="top"></a>

    
    


<a name="wp1074613"> </a><h1 class="pTitle">
About Interop Mode

</h1>
<a name="wp1074614"> </a><p class="pBody">
Cisco NX-OS software supports the following four interop modes:

</p>
<div class="pSmartList1"><ul class="pSmartList1">
<a name="wp1074615"> </a><li class="pSmartList1">Mode 1&#8212; Standards based interop mode that requires all other vendors in the fabric to be in interop 
mode.
</li>
<a name="wp1074617"> </a><li class="pSmartList1">Mode 2&#8212;Brocade native mode (Core PID 0).
</li>
<a name="wp1074618"> </a><li class="pSmartList1">Mode 3&#8212;Brocade native mode (Core PID 1).
</li>
<a name="wp1074620"> </a><li class="pSmartList1">Mode 4&#8212;McData native mode.
</li>
</ul></div>
<a name="wp1074621"> </a><p class="pBody">
For information about configuring interop modes 2, 3, and 4, refer to the <em class="cEmphasis">Cisco MDS 9000 Family 
Switch-to-Switch Interoperability Configuration Guide</em>.

</p>
<a name="wp1074625"> </a><p class="pBody">
<a href="adv12.html#wp1074632">Table&#160;28-2</a> lists the changes in switch behavior when you enable interoperability mode. These changes 
are specific to switches in the Cisco MDS 9000 Family while in interop mode.

</p>
<a name="wp1093485"> </a><p class="pBodyRelative">
</p><div>
<table border="2" cellpadding="2" id="wp1074632table1074626">
  <caption><a name="wp1074632"> </a><div class="pTableTitle">
Table&#160;28-2	Changes in Switch Behavior When Interoperability Is Enabled&#160;

</div>
</caption>
  <tr bgcolor="#CCCCCC" align="left" valign="middle">    <th><a name="wp1074636"> </a><p class="pCellHeading">
Switch Feature

</p>
</th>
    <th><a name="wp1074638"> </a><p class="pCellHeading">
Changes if Interoperability Is Enabled

</p>
</th>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074641"> </a><p class="pBody">
Domain IDs

</p>
</td>
    <td><a name="wp1074643"> </a><p class="pBody">
Some vendors cannot use the full range of 239 domains within a fabric.

</p>
<a name="wp1074644"> </a><p class="pBody">
Domain IDs are restricted to the range 97-127. This is to accommodate 
McData’s nominal restriction to this same range. They can either be set up 
statically (the Cisco MDS switch accept only one domain ID, if it does not get 
that domain ID it isolates itself from the fabric) or preferred. (If it does not get 
its requested domain ID, it accepts any assigned domain ID.)

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074646"> </a><p class="pBody">
Timers

</p>
</td>
    <td><a name="wp1074648"> </a><p class="pBody">
All Fibre Channel timers must be the same on all switches as these values are 
exchanged by E ports when establishing an ISL. The timers are F_S_TOV, 
D_S_TOV, E_D_TOV, and R_A_TOV.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074651"> </a><p class="pBody">
F_S_TOV

</p>
</td>
    <td><a name="wp1074653"> </a><p class="pBody">
Verify that the Fabric Stability Time Out Value timers match exactly. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074655"> </a><p class="pBody">
D_S_TOV

</p>
</td>
    <td><a name="wp1074657"> </a><p class="pBody">
Verify that the Distributed Services Time Out Value timers match exactly.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074659"> </a><p class="pBody">
E_D_TOV

</p>
</td>
    <td><a name="wp1074661"> </a><p class="pBody">
Verify that the Error Detect Time Out Value timers match exactly.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074663"> </a><p class="pBody">
R_A_TOV

</p>
</td>
    <td><a name="wp1074665"> </a><p class="pBody">
Verify that the Resource Allocation Time Out Value timers match exactly.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074668"> </a><p class="pBody">
Trunking

</p>
</td>
    <td><a name="wp1074670"> </a><p class="pBody">
Trunking is not supported between two different vendor’s switches. This 
feature may be disabled on a per port or per switch basis.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074673"> </a><p class="pBody">
Default zone 

</p>
</td>
    <td><a name="wp1074675"> </a><p class="pBody">
The default zone behavior of permit (all nodes can see all other nodes) or deny 
(all nodes are isolated when not explicitly placed in a zone) may change.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074678"> </a><p class="pBody">
Zoning attributes

</p>
</td>
    <td><a name="wp1074680"> </a><p class="pBody">
Zones may be limited to the pWWN and other proprietary zoning methods 
(physical port number) may be eliminated.

</p>
<a name="wp1074681"> </a><p class="pBodyAutonumNoRule">
<strong>Note	&nbsp;&nbsp;&nbsp;</strong> Brocade uses the <b class="cBold">cfgsave</b> command to save fabric-wide zoning 
configuration. This command does not have any effect on Cisco MDS 
9000 Family switches if they are part of the same fabric. You must 
explicitly save the configuration on each switch in the Cisco MDS 9000 
Family.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074683"> </a><p class="pBody">
Zone propagation

</p>
</td>
    <td><a name="wp1074685"> </a><p class="pBody">
Some vendors do not pass the full zone configuration to other switches, only 
the active zone set gets passed. 

</p>
<a name="wp1074686"> </a><p class="pBody">
Verify that the active zone set or zone configuration has correctly propagated 
to the other switches in the fabric.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074689"> </a><p class="pBody">
VSAN

</p>
</td>
    <td><a name="wp1074691"> </a><p class="pBody">
Interop mode only affects the specified VSAN.

</p>
<a name="wp1074693"> </a><p class="pBodyAutonumNoRule">
<strong>Note	&nbsp;&nbsp;&nbsp;</strong> Interop modes cannot be enabled on FICON-enabled VSANs.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074696"> </a><p class="pBody">
TE ports and 
PortChannels

</p>
</td>
    <td><a name="wp1074699"> </a><p class="pBody">
TE ports and PortChannels cannot be used to connect Cisco MDS to non-Cisco 
MDS switches. Only E ports can be used to connect to non-Cisco MDS 
switches. TE ports and PortChannels can still be used to connect an Cisco MDS 
to other Cisco MDS switches even when in interop mode. 

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074702"> </a><p class="pBody">
FSPF

</p>
</td>
    <td><a name="wp1074704"> </a><p class="pBody">
The routing of frames within the fabric is not changed by the introduction of 
interop mode. The switch continues to use src-id, dst-id, and ox-id to load 
balance across multiple ISL links.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074706"> </a><p class="pBody">
Domain 
reconfiguration 
disruptive

</p>
</td>
    <td><a name="wp1074708"> </a><p class="pBody">
This is a switch-wide impacting event. Brocade and McData require the entire 
switch to be placed in offline mode and/or rebooted when changing domain 
IDs.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074710"> </a><p class="pBody">
Domain 
reconfiguration 
nondisruptive

</p>
</td>
    <td><a name="wp1074712"> </a><p class="pBody">
This event is limited to the affected VSAN. Only Cisco MDS 9000 Family 
switches have this capability&#8212;only the domain manager process for the 
affected VSAN is restarted and not the entire switch.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074715"> </a><p class="pBody">
Name server

</p>
</td>
    <td><a name="wp1074717"> </a><p class="pBody">
Verify that all vendors have the correct values in their respective name server 
database.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1074719"> </a><p class="pBody">
IVR

</p>
</td>
    <td><a name="wp1074721"> </a><p class="pBody">
IVR-enabled VSANs can be configured in<b class="cBold"> no interop</b> (default) mode or in any 
of the <b class="cBold">interop</b> modes.

</p>
</td>
</tr>
</table>
</div>
<p class="pBodyRelative">
</p>
<hr /><br><p class="pBody">Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.</p> 

    </blockquote>

  </body>
</html>
