> # Configuring Persistent FC IDs

> ## Detailed Steps

> To configure persistent FC IDs, follow these steps:

> 1. Expand Fabric > All VSANs and then select Domain Manager in the Logical Domains pane for the fabric and VSAN that you want to configure the Persistent FC ID list for.

> You see the running configuration of the domain in the Information pane.

> 2. Click the Persistent FcIds tab and click Create Row.
> 3. Select the switch, WWN, and FC ID that you want to make persistent.
> 4. Set the Mask radio button to single or area.
> 5. Set the Assignment radio button to static or dynamic.
> 6. Click the Apply Changes icon to save these changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.