> # Creating CFS Regions

> ## Detailed Steps

> To create a CFS region, follow these steps:

> 1. Expand Switches and select CFS from the Physical Attributes pane.

> The information pane displays the Global, IP Multicast, Feature by Region, and All Regions tabs.

> 2. Click the All Regions tab.

> The tab displays a list of Switches and RegionIds.

> 3. Click the Create Row button on the toolbar.
> 4. From the drop-down list, select the switch and choose a RegionId from the range.
> 5. Click Create.

> Upon successful creation of the region, Success is displayed at the bottom of the dialog box.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.