> # FSPF General

> Field | Description
> --- | ---
> AdminStatus | The desired state of FSPF on this VSAN.
> OperStatus | State of FSPF on this VSAN.
> SetToDefault | Enabling this changes each value in this row to its default value. If all the configuration parameters have their default values and if the VSAN is suspended, then the row is deleted automatically.
> RegionId | The autonomous region of the local switch on this VSAN.
> DomainId | The domain ID of the local switch on this VSAN.
> SpfHoldTime | The minimum time between two consecutive SPF computations on this VSAN. The smaller value means that routing will react to the changes faster but the CPU usage is greater.
> SpfDelay | The time between when FSPF receives topology updates and when it starts the Shortest Path First (SPF) computation on this VSAN. The smaller value means that routing will react to the changes faster but the CPU usage is greater.
> MinLsArrival | The minimum time after accepting a Link State Record (LSR) on this VSAN before accepting another update of the same LSR on the same VSAN. An LSR update that is not accepted because of this time interval is discarded.
> MinLsInterval | The minimum time after this switch sends an LSR on this VSAN before it will send another update of the same LSR on the same VSAN.
> LsRefreshTime | The interval between transmission of refresh LSRs on this VSAN.
> LSRMaxAge | The maximum age an LSR will be retained in the FSPF database on this VSAN. It is removed from the database after MaxAge is reached.
> CreateTime | When this entry was last created.
> CheckSum | The total checksum of all the LSRs on this VSAN.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.