> # Enabling DHCHAP

> To enable DHCHAP for a Cisco MDS switch , follow these steps:

> 1. Expand Switches, expand Security and then select FC-SP.

> The Control tab is the default. You see the FC-SP enable state for all switches in the fabric.

> 2. Set the Command drop-down menu to enable for all switches that you want to enable FC-SP on.
> 3. Click the Apply Changes icon to enable FC-SP and DHCHAP on the selected switches.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.