> # Adding Zone Members

> Once you create a zone, you can add members to the zone. You can add members using multiple port identification types.

> ## Detailed Steps

> To add a member to a zone, follow these steps:

> 1. Choose Zone > Edit Local Full Zone Database.

> You see the Select VSAN dialog box.

> 2. Select a VSAN and click OK.

> You see the Edit Local Full Zone Database dialog box for the selected VSAN.

> 3. Select the members you want to add from the Fabric pane and click Add to Zone or click the zone where you want to add members and click the Insert icon.

> You see the Add Member to Zone dialog box.

> Note The Device Alias radio button is visible only if device alias is in enhanced mode. For more information, see "Creating Device Aliases" topic.

> 4. Click the browse button and select a port name or check the LUN check box and click the browse button to configure LUNs.
> 5. Select the options for Device Type field. You can select any one of the options: Host, Storage, or Both.
> 6. Click Add to add the member to the zone.

> Note When configuring a zone member, you can specify that a single LUN has multiple IDs depending on the operating system. You can select from six different operating systems.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.