<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<!-- saved from url=(0014)about:internet -->
<html xmlns="http://www.w3.org/1999/xhtml" xml:lang="en" lang="en">
  <head>
    <meta http-equiv="Content-Type" content="text/html; charset=UTF-8" />
    <meta http-equiv="Content-Style-Type" content="text/css" />
    <meta name="GENERATOR" content="Quadralay WebWorks AutoMap 2003 Platinum Edition Client for FrameMaker 8.6.6597.0" />
    <meta name="TEMPLATEBASE" content="emwebh8-1-17" />
    <meta name="LASTUPDATED" content="08/01/13 14:45:16" />
    <title>Port Monitoring Traffic (9020) </title>
    <!-- Copyright 2010-2013, Cisco Systems, Inc. All rights reserved. -->

    <link rel="StyleSheet" href="document.css" type="text/css" />
    <link rel="StyleSheet" href="catalog.css" type="text/css" />


<script> 
    var is_chrome = navigator.userAgent.toLowerCase().indexOf('chrome') > -1; 
   
    if(is_chrome){document.domain=document.domain}
   </script>
    <script type="text/javascript" language="JavaScript1.2" src="expand.js"></script>
    <script type="text/javascript" language="JavaScript1.2" src="page.js"></script>

    <script type="text/javascript" language="JavaScript1.2">
     <!--
      function  WWNoOp() {}
      function  WWNoValue() { return ""; }

      var  VarDropDown;

      if (typeof(HTMLHelp_Object) != "undefined")
      {
        VarDropDown = new WWDropDown_Object();
      }
      else
      {
        VarDropDown = new Object();
        VarDropDown.fAnchorOpen  = WWNoOp;
        VarDropDown.fAnchorClose = WWNoOp;
        VarDropDown.fDIVOpen  = WWNoOp;
        VarDropDown.fDIVClose = WWNoOp;
      }
     // -->
    </script>

  
<SCRIPT language="javascript">
<!--
  self.document.write("<link href='"+top.relPath+"shared/style.css' rel='stylesheet' type='text/css'>");
  myid=376;
  self.document.write("<script type='text/javascript' language='JavaScript' src='"+top.relPath+"shared/con_utils.js'></scr"+"ipt>");
//-->
</SCRIPT>
</head>

  <body onload="highlightSearchTerms();" bgcolor="#ffffff">

    
    <blockquote>
    <a name="top"></a>

    
    


<a name="wp1052270"> </a><h1 class="pTitle">
Port Monitoring Traffic (9020)




</h1>
<a name="wp1052308"> </a><p class="pBodyRelative">
</p><div>
<table border="2" cellpadding="2" id="wp1052273table1052271">
  <caption></caption>
  <tr bgcolor="#CCCCCC" align="left" valign="middle">    <th><a name="wp1052273"> </a><p class="pCellHeading">
Field 

</p>
</th>
    <th><a name="wp1052275"> </a><p class="pCellHeading">
Description 

</p>
</th>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052277"> </a><p class="pBody">
Rx bytes

</p>
</td>
    <td><a name="wp1052279"> </a><p class="pBody">
The number of frames/packets/IOs/etc that have been received by this 
port. A Fibre Channel frame starts with SOF and ends with EOF. FC 
loop devices should not count frames passed through. This value 
represents the sum total for all other Rx objects

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052281"> </a><p class="pBody">
Tx bytes

</p>
</td>
    <td><a name="wp1052283"> </a><p class="pBody">
The number of octets or bytes that have been transmitted by this port. 
One second periodic polling of the port. This value is saved and 
compared with the next polled value to compute net throughput. For 
Fibre Channel ordered sets are not included in the count.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052285"> </a><p class="pBody">
Rx frames

</p>
</td>
    <td><a name="wp1052287"> </a><p class="pBody">
The number of octets or bytes that have been received by this port. One 
second periodic polling of the port. This value is saved and compared 
with the next polled value to compute net throughput. For Fibre 
Channel, ordered sets are not included in the count.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052289"> </a><p class="pBody">
Tx frames

</p>
</td>
    <td><a name="wp1052291"> </a><p class="pBody">
The number of octets or bytes that have been transmitted by this port. 
One second periodic polling of the port. This value is saved and 
compared with the next polled value to compute net throughput. For 
Fibre Channel, ordered sets are not included in the count.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052293"> </a><p class="pBody">
Class2 Rx frames

</p>
</td>
    <td><a name="wp1052295"> </a><p class="pBody">
Count of Class 2 Frames received at this port. This is a Fibre Channel 
only statistic.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052297"> </a><p class="pBody">
Class2 Tx frames

</p>
</td>
    <td><a name="wp1052299"> </a><p class="pBody">
Count of Class 2 Frames transmitted out this port. This is a Fibre 
Channel only statistic.

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052301"> </a><p class="pBody">
Class3 Rx frames

</p>
</td>
    <td><a name="wp1052303"> </a><p class="pBody">
Count of Class 3 Frames received at this port. This is a Fibre Channel 
only statistic

</p>
</td>
</tr>
  <tr align="left" valign="top">    <td><a name="wp1052305"> </a><p class="pBody">
Class3 Tx frames

</p>
</td>
    <td><a name="wp1052307"> </a><p class="pBody">
Count of Class 3 Frames transmitted out this port. This is a Fibre 
Channel only statistic.

</p>
</td>
</tr>
</table>
</div>
<p class="pBodyRelative">
</p>
<hr /><br><p class="pBody">Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.</p> 

    </blockquote>

  </body>
</html>
