## Connect New Border leaf to the Edge Router

1. From the menu bar, select Config > Border Leaf Device Pairing.

2. Click Add. Select Border Leaf.

3. Define the parameters for the Border leaf configuration and edge router configuration for pairing.

Field | Description
Name | Select the name from the drop-down list for the Border leaf.
IP Address | The IP address is auto-populated based on the selected Border Leaf.
Port Channel or the Interface Name | Specify the interface name or port channel between Border Leaf and Edge Router.
Maximum Number of Partitions | Specifies the number of partitions required for the configuration
Default Profile Name | Select the default profile name from the drop-down list to apply for the profile.
Notify Border Leaf when relevant partitions | Select to notify the Border Leaf when relevant partitions are created.

4. Click OK to connect the new border leaf device to the Edge router.