> # NTP General

> Field | Description
> --- | ---
> Leap | Two-bit code warning of an impending leap second to be inserted in the NTP timescale.
> RootDelay | A signed fixed-point number indicating the total round-trip delay in seconds, to the primary reference source at the root of the synchronization subnet.
> RootDispersion | The maximum error in seconds, relative to the primary reference source at the root of the synchronization subnet.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.